1. Install the OS to your TF Card
2. Download the file named: mzp280qv1t-v2

from <https://github.com/iUniker/mzp280qv1t-v2>

1. Copy mzp280qv1t-v2 to the same directory as config.txt
2. Open config.txt , and add

[all]

include mzp280qv1t-v2.txt

to the bottom of the file.

1. Save and quit.
2. Insert the card to your Pi, and reboot, the screen will work.